skip to main | skip to sidebar

# EEE Journal

EEE PC, MSI Wind, MiniNote mods, hacks and tuning, benchmark, news, review and tips. Resources for ultra portable laptops and subnotebooks.

Blogger Template by Blogcrowds

## Sunday, May 11, 2008

### EEE PC - CPU for 700, 701 and 900

There is a lot of confusion about the EEE PC CPU, especially about CPU clock and cache size.
All models released so far use an Intel Celeron-M ULV (Ultra Low Voltage), model 353.
CPU Cache (from the Celeron M 353 datasheet) :

- 32KB L1 instruction + 32KB L1 data cache (write back)
- 512KB L2 cache

CPU frequency

- EEE PC 700 (2G) : 571 MHz (from original 800 MHz)
- EEE PC 701 (4G, 8G) : 630 MHz (from original 900 MHz)
- EEE PC 900 : the original 900 MHz

Front Side Bus: 400 MHz (original...)
It is possible (and you void the guarrantee!) to overclocking the CPU and/or replace the CPU with a Pentium-M ULV.
Newer Post Older Post Home